**Marking scheme – Skill Carpentry – 26**

1. Overall length should be 600mm 10
2. Overall width should be 300mm 10
3. Overall width of back should be 219mm 10
4. Measurements of joint as per drawing 10
5. Face marking 10
6. Joints before gluing 15
7. Joints after gluing 15
8. Bottom ply fixed 10
9. Extra material 1

Total = 100